Personal notes

Battery voltage adc does not seem to be dropping as the battery voltage drops.

Potential issue is that RS4485 requests the string before the adc has been converted into mV!!!

Will run a test to confirm whether it is the timing or not

Information, it takes just over 18 seconds from power on to the 0x07 RS485 command being sent.