Personal notes

Information, it takes just over 18 seconds from power on to the 0x07 RS485 command being sent.

Change the code and the order that each sense circuit is read.

Use all the same length wires to each sense circuit.